(footprint "WE-MAPI_4020"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.485 0)
		(layer "F.SilkS")
		(uuid "9bbdb9fc-3a4b-4284-9c60-0e3a9a29c831")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WE-MAPI_4020"
		(at 0 3.365 0)
		(layer "F.Fab")
		(uuid "24cd193e-fa8d-454f-b87b-febe30b5c160")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "dca77de0-135e-457c-abbc-47841acdcdf8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0b5e96b3-95e2-460d-8af2-f7291b3946e3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center -2.8 -2)
		(end -2.7 -2)
		(stroke
			(width 0.3)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "9f62d14f-fdf2-42ef-a133-b7d22098e6d4")
	)
	(fp_poly
		(pts
			(xy -2.35 -2.35) (xy 2.35 -2.35) (xy 2.35 2.35) (xy -2.35 2.35)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.CrtYd")
		(uuid "0b673fa6-223e-42c3-aff8-0a4d63cf6e95")
	)
	(fp_line
		(start -2.15 -2.15)
		(end 2.15 -2.15)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bf0a8545-4b51-4168-84be-f112932dae48")
	)
	(fp_line
		(start -2.15 2.15)
		(end -2.15 -2.15)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "539966bb-6d12-4234-b0de-5bb035ea6e04")
	)
	(fp_line
		(start -2.05 -2.05)
		(end 2.05 -2.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "774aace2-007d-443b-bc04-471c25471804")
	)
	(fp_line
		(start -2.05 2.05)
		(end -2.05 -2.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b60cf9bf-dfd5-4a4a-8703-d0e7e0858cc6")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 2.05 2.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "22ca5068-bde5-42d2-9e81-6e04f06106af")
	)
	(fp_line
		(start 2.05 2.05)
		(end -2.05 2.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "57e62d84-3b8e-454f-a0a8-fdc495cbcacd")
	)
	(fp_line
		(start 2.15 -2.15)
		(end 2.15 2.15)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aa564eff-74b3-4199-9b2e-caf12f9eeaf9")
	)
	(fp_line
		(start 2.15 2.15)
		(end -2.15 2.15)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "73e1482e-5e52-4dfd-866d-9f6801a182a2")
	)
	(pad "1" smd rect
		(at -1.185 0)
		(size 0.98 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "caa41985-6dcd-4c5c-9c26-132a92d80cfc")
	)
	(pad "2" smd rect
		(at 1.185 0)
		(size 0.98 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "7bfa217d-3655-47bd-a279-362b0bec16a9")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "ea3868b1-bb43-4a52-927d-9a09c04ee75e")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -0.695 -1.85) (xy 0.695 -1.85) (xy 0.695 1.85) (xy -0.695 1.85)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "179d4236-b6d6-4ff8-a0a1-8807ba155185")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -0.695 -1.85) (xy 0.695 -1.85) (xy 0.695 1.85) (xy -0.695 1.85)
			)
		)
	)
	(embedded_fonts no)
	(model "/Users/christianratcliffe/Dropbox/Christian's/MyKiCadLibraries/3DModels/M8/WE-MAPI_4020.step"
		(offset
			(xyz 0 0 2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 -0 -0)
		)
	)
)
