(footprint "150060RS75003"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "<B>WL-SMCW SMT Mono-color Chip LED Waterclear<Br><Br></B>Size: 0603, SMT, 2pins<Br>1.6x0.8x0.7mm(LXWXH)")
	(property "Reference" "REF**"
		(at 0 -1.4064 0)
		(layer "F.SilkS")
		(uuid "31c97d84-9951-4cbb-a857-2cacda13eb39")
		(effects
			(font
				(size 0.64 0.64)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WL-SMCW_0603_ADVANCE"
		(at 0 1.2936 0)
		(layer "F.Fab")
		(uuid "ed30abb6-9a46-4faf-804c-61f47b2c0910")
		(effects
			(font
				(size 0.64 0.64)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "13c666f0-5c94-4989-8be1-2c5975586ba7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "37e15cbc-bd13-4a0e-a9f1-c6b5092ec4eb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.13 0)
		(end 0.11 -0.14)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e6a8dbd4-bad2-4524-b965-5e722dc597d1")
	)
	(fp_line
		(start -0.1 -0.5)
		(end 0.1 -0.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6b4d4333-5219-44a3-84f8-37e87a63b216")
	)
	(fp_line
		(start 0.1 0.5)
		(end -0.1 0.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e5c08bc-c270-4aeb-8071-03c5ca854621")
	)
	(fp_line
		(start 0.11 -0.14)
		(end 0.11 0.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "32a06561-a04c-4549-ae05-11219375b74b")
	)
	(fp_line
		(start 0.11 0.15)
		(end -0.13 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c03804af-bd2a-4146-82dc-dbccd1a91cb0")
	)
	(fp_poly
		(pts
			(xy -1.4 -0.7) (xy 1.4 -0.7) (xy 1.4 0.7) (xy -1.4 0.7)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.CrtYd")
		(uuid "d35b279b-6df3-4b12-84fb-abdcddefdb94")
	)
	(fp_line
		(start -0.8 -0.4)
		(end 0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "48db7758-6e6b-4897-a206-f05cd90f7efd")
	)
	(fp_line
		(start -0.8 0.4)
		(end -0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "09ddde68-f5cf-49fd-b845-d844b7b1a7f3")
	)
	(fp_line
		(start -0.8 0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4a81c317-8a6b-49a4-9d0b-0c31795c365a")
	)
	(fp_line
		(start -0.13 0)
		(end 0.11 0.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "847be69d-9424-440a-9900-a8c17ca8d7ec")
	)
	(fp_line
		(start 0.11 -0.14)
		(end -0.13 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a8b33774-250a-46e9-ba76-8fdc37083a1d")
	)
	(fp_line
		(start 0.11 0.15)
		(end 0.11 -0.14)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fbcf11cd-fd01-45f5-9c58-ecc6dccf194b")
	)
	(fp_line
		(start 0.8 -0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "53134150-e4eb-4507-aaa9-fdbbf85eb7fa")
	)
	(fp_text user "+"
		(at -1.5 0.3 0)
		(layer "F.SilkS")
		(uuid "491c9c0c-9b8a-4087-a5ea-982616ff24e8")
		(effects
			(font
				(size 0.48 0.48)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "+"
		(at -1.5 0.3 0)
		(layer "F.Fab")
		(uuid "28f8e767-ebf1-4ad9-80b4-52f763af57fd")
		(effects
			(font
				(size 0.48 0.48)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.8 0)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "dc23281a-cbe1-4f24-9c22-a2065ecd502e")
	)
	(pad "2" smd rect
		(at 0.8 0)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "32158a28-ec57-46f2-b49f-83bf1268b7ad")
	)
	(embedded_fonts no)
	(model "/Users/christianratcliffe/Dropbox/Christian's/MyKiCadLibraries/3DModels/M8/150060RS75003.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 180)
		)
	)
)
